Contents

[**Cisco IP Conference Phone 7832 Release Notes for Firmware Release 14.2(1)SR2** 3](#_Toc152162750)

[**New and Changed Features** 3](#_Toc152162751)

[**Features Available with the Firmware Release** 3](#_Toc152162752)

[**Configurable DNS when DHCP is on** 3](#_Toc152162753)

[**Caveats** 3](#_Toc152162754)

[**View Caveats** 3](#_Toc152162755)

[**Cisco IP Phone Firmware Support Policy** 3](#_Toc152162756)

**Cisco IP Conference Phone 7832 Release Notes for Firmware Release 14.2(1)SR2**

These release notes support the Cisco IP Phone 7832 running SIP Firmware Release 14.2(1)SR2.

**New and Changed Features**

**Features Available with the Firmware Release**

The following sections describe the features available with the Firmware Release.

**Configurable DNS when DHCP is on**

With this feature enhancement, the end users can modify the DNS address on the phone when DHCP is on. After a network reset in the phone menu, the DNS address will be reset and the phone will then automatically get a DNS address from the DHCP server.

**Caveats**

**View Caveats**

We report open and resolved customer-found bugs of severity 1 to 3. You can find details about listed bugs and search for other bugs by using the Cisco Bug Search Tool. For more info on using the Bug Search, see [Bug Search Tool Help](https://www.cisco.com/c/en/us/support/web/tools/bst/bsthelp/index.html).

* Use this URL for all caveats: <https://bst.cloudapps.cisco.com/bugsearch/search?kw=&pf=prdNm&pfVal=284883944&rls=14.2(1)SR2&sb=anfr&svr=3nH&bt=custV>
* Use this URL for all open caveats:

<https://bst.cloudapps.cisco.com/bugsearch/search?kw=&pf=prdNm&pfVal=284883944&rls=14.2(1)SR2&sb=afr&sts=open&svr=3nH&bt=custV>

* Use this URL for all resolved caveats: <https://bst.cloudapps.cisco.com/bugsearch/search?kw=&pf=prdNm&pfVal=284883944&rls=14.2(1)SR2&sb=fr&svr=3nH&bt=custV>

**Cisco IP Phone Firmware Support Policy**

For information on the support policy for phones, see <https://cisco.com/go/phonefirmwaresupport>.

